Eigenschaften von Messstellen

| ALPHA-VISION®job.dbf

### Eigenschaften von Messstellen

Eigenschaft | Beschreibung | Rückgabe-Typ | Rückgabewert

AlarmAct

Actual alarm status

int

Bits 0...6 Level / Status:
0...15 Alarmlevel des akt. Status
16 Out of range
17 Undefined
18 Faded out
64 Blocked
Bit 7 unquittiert
128...143 Unquittiert + akt. Alarmlevel
alle Bitgruppen können in bel. Kombinationen untereinander auftreten

AlDispl | Alarm Ident display | string | 6 Zeichen
AlVideo | Alarm ident video | string | 6 Zeichen
ArchOvfl | Archive change to overflow | bool | 0 / 1
ArchSts1 | Archive change to status 1 | bool | 0 / 1
ArchSts2 | Archive change to status 2 | bool | 0 / 1
ArchSts3 | Archive change to status 3 | bool | 0 / 1
ArchSts4 | Archive change to status 4 | bool | 0 / 1
ArchSts5 | Archive change to status 5 | bool | 0 / 1
ArchSts6 | Archive change to status 6 | bool | 0 / 1
ArchSts7 | Archive change to status 7 | bool | 0 / 1
ArchSts8 | Archive change to status 8 | bool | 0 / 1
AudAlStsAct | Actual audible alarm group | int | 0...63
AudAlOvfl | Audible alarm grp overflow | int | 0...63
AudAlSts1 | Audible alarm grp status 1 | int | 0...63
AudAlSts2 | Audible alarm grp status 2 | int | 0...63
AudAlSts3 | Audible alarm grp status 3 | int | 0...63
AudAlSts4 | Audible alarm grp status 4 | int | 0...63
AudAlSts5 | Audible alarm grp status 5 | int | 0...63
AudAlSts6 | Audible alarm grp status 6 | int | 0...63
AudAlSts7 | Audible alarm grp status 7 | int | 0...63
AudAlSts8 | Audible alarm grp status 8 | int | 0...63
Comment | Comment | string | 20 Zeichen
CompPointId | Compensation point ID | string | 6 Zeichen
DelOvflIn | Time delay into status 0 (out of range) | int | 0 sec...3600sec
DelOvflOut | Time delay out of status 0 (out of range) | int | 0 sec...3600sec
DelSts1In | Time delay into status 1 | int | 0 sec ...3600 sec
DelSts1Out | Time delay out of status1 | int | 0 sec ...3600 sec
DelSts2In | Time delay into status 2 | int | 0 sec ...3600 sec
DelSts2Out | Time delay out of status2 | int | 0 sec ...3600 sec
DelSts3In | Time delay into status 3 | int | 0 sec ...3600 sec
DelSts3Out | Time delay out of status3 | int | 0 sec ...3600 sec
DelSts4In | Time delay into status 4 | int | 0 sec ...3600 sec
DelSts4Out | Time delay out of status4 | int | 0 sec ...3600 sec
DelSts5In | Time delay into status 5 | int | 0 sec ...3600 sec
DelSts5Out | Time delay out of status5 | int | 0 sec ...3600 sec
DelSts6In | Time delay into status 6 | int | 0 sec ...3600 sec
DelSts6Out | Time delay out of status6 | int | 0 sec ...3600 sec
DelSts7In | Time delay into status 7 | int | 0 sec ...3600 sec
DelSts7Out | Time delay out of status7 | int | 0 sec ...3600 sec
DelSts8In | Time delay into status 8 | int | 0 sec ...3600 sec
DelSts8Out | Time delay out of status8 | int | 0 sec ...3600 sec
DynLim1 | Dynamic limit grp 1 | int | 0...999
DynLim2 | Dynamic limit grp 2 | int | 0...999
DynLim3 | Dynamic limit grp 3 | int | 0...999
DynLim4 | Dynamic limit grp 4 | int | 0...999
DynLim5 | Dynamic limit grp 5 | int | 0...999
DynLim6 | Dynamic limit grp 6 | int | 0...999
DynLim7 | Dynamic limit grp 7 | int | 0...999
FNumAck | Accessno. for acknowledge | int | 0...99
FNumPara | Accessno. for param change | int | 0...99
HasHistory | Value Recording flag | bool | 0 / 1
HitiId | Hints & tips Id | string | 6 Zeichen
HystLimit | Hysteresis for limits | int / float | 32bit im entspr. Werteformat
HystUpdate | Hysteresis for value update | int / float | 32bit im entspr. Werteformat
InhOvfl | Inhibit group for status 0 (outof range) | int | 0...999
InhStsAct | actual inhibit group | int | 0...999
InhSts1 | Inhibit group for status 1 | int | 0...999
InhSts2 | Inhibit group for status 2 | int | 0...999
InhSts3 | Inhibit group for status 3 | int | 0...999
InhSts4 | Inhibit group for status 4 | int | 0...999
InhSts5 | Inhibit group for status 5 | int | 0...999
InhSts6 | Inhibit group for status 6 | int | 0...999
InhSts7 | Inhibit group for status 7 | int | 0...999
InhSts8 | Inhibit group for status 8 | int | 0...999
IsInhSts1 | Is state 1 inhibited ? | bool | 0 / 1
IsInhSts2 | Is state 2 inhibited ? | bool | 0 / 1
IsInhSts3 | Is state 3 inhibited ? | bool | 0 / 1
IsInhSts4 | Is state 4 inhibited ? | bool | 0 / 1
IsInhSts5 | Is state 5 inhibited ? | bool | 0 / 1
IsInhSts6 | Is state 6 inhibited ? | bool | 0 / 1
IsInhSts7 | Is state 7 inhibited ? | bool | 0 / 1
IsInhSts8 | Is state 8 inhibited ? | bool | 0 / 1
Limit1 | Limit 1 (to status 2) | int / float | 32bit im entspr. Werteformat
Limit2 | Limit 2 (to status 3) | int / float | 32bit im entspr. Werteformat
Limit3 | Limit 3 (to status 4) | int / float | 32bit im entspr. Werteformat
Limit4 | Limit 4 (to status 5) | int / float | 32bit im entspr. Werteformat
Limit5 | Limit 5 (to status 6) | int / float | 32bit im entspr. Werteformat
Limit6 | Limit 6 (to status 7) | int / float | 32bit im entspr. Werteformat
Limit7 | Limit 7 (to status 8) | int / float | 32bit im entspr. Werteformat
LvlAct | Actualalarm level | int | 0...15
LvlOvfl | Alarm level status 0 (out of range) | int | 0...15
LvlSts1 | Alarm level for status 1 | int | 0...15
LvlSts2 | Alarm level for status 2 | int | 0...15
LvlSts3 | Alarm level for status 3 | int | 0...15
LvlSts4 | Alarm level for status 4 | int | 0...15
LvlSts5 | Alarm level for status 5 | int | 0...15
LvlSts6 | Alarm level for status 6 | int | 0...15
LvlSts7 | Alarm level for status 7 | int | 0...15
LvlSts8 | Alarm level for status 8 | int | 0...15
PrnOvfl | Print out change to overflow | bool | 0 / 1
PrnSts1 | Print out change to status 1 | bool | 0 / 1
PrnSts2 | Print out change to status 2 | bool | 0 / 1
PrnSts3 | Print out change to status 3 | bool | 0 / 1
PrnSts4 | Print out change to status 4 | bool | 0 / 1
PrnSts5 | Print out change to status 5 | bool | 0 / 1
PrnSts6 | Print out change to status 6 | bool | 0 / 1
PrnSts7 | Print out change to status 7 | bool | 0 / 1
PrnSts8 | Print out change to status 8 | bool | 0 / 1
Range | Measuring-Range | int /float | 5 Zeichen
RangeEnd | Measuring-Range to | int / float | 32bit im entspr. Werteformat
RangeStart | Measuring-Range from | int / float | 32bit im entspr. Werteformat/TD>
RawAddr | PLC- I/O-Address | string | 13 Zeichen
RecHistory | Value Recording status | bool | 0 / 1
Remark | Var. Text Remark | string | 30
ScaleGrp | Scaling group | int | 0...63
ScanCycle | Scan cycle | int | 0...99
Sensor | Transmitter name | string | 12 Zeichen
SgnlStsAct | Actual signal output | int | 0...63
SgnlOvfl | Signal output overflow | int | 0...63
SgnlSts1 | Signal output status 1 | int | 0...63
SgnlSts2 | Signal output status 2 | int | 0...63
SgnlSts3 | Signal output status 3 | int | 0...63
SgnlSts4 | Signal output status 4 | int | 0...63
SgnlSts5 | Signal output status 5 | int | 0...63
SgnlSts6 | Signal output status 6 | int | 0...63
SgnlSts7 | Signal output status 7 | int | 0...63
SgnlSts8 | Signal output status 8 | int | 0...63
SimuFreeze | Freeze simulation status | bool | 0 / 1
SimuParam1 | Simulation parameter 1 | int / float | 32bit im entspr. Werteformat
SimuParam2 | Simulation parameter 2 | int / float | 32bit im entspr. Werteformat

SimuType

Simulation type

int

0 no simulation
1 Sprungfunktion
2 Rampenfunktion
3 PT1
4 Festwert Simulation

Slot | Slot | string | 8 Zeichen
Station | Target station | string | 5 Zeichen

Status

Actual status

int

Bits 0...4 Status:
0 uninitialisiert
1 closed / < limit 1
2 opened / < limit 2
3 < limit 3
4 < limit 4
5 < limit 5
6 < limit 6
7 < limit 7
8 > limit 7
16 OutOfRange
17 Undefined
18 FadedOut
Bit 5 Failure
Bit 6 Blocked
Bit 7 Unquittiert
Bits 8...31 unbenutzt, = 0
alle Bitgruppen können in bel. Kombinationen untereinander auftreten

TechId | TechnologicalId | string | 2 Zeichen
TxtOvfl | Status text for status 0 (out ofrange) | string | 10 Zeichen
TxtStsAct | Actual status text | string | 10 Zeichen
TxtSts1 | Status text for status 1 | string | 10 Zeichen
TxtSts2 | Status text for status 2 | string | 10 Zeichen
TxtSts3 | Status text for status 3 | string | 10 Zeichen
TxtSts4 | Status text for status 4 | string | 10 Zeichen
TxtSts5 | Status text for status 5 | string | 10 Zeichen
TxtSts6 | Status text for status 6 | string | 10 Zeichen
TxtSts7 | Status text for status 7 | string | 10 Zeichen
TxtSts8 | Status text for status 8 | string | 10 Zeichen
UndefGrp | Undefined group | int | 0...999
Unit | Unit | string | 5 Zeichen
VisAlOvfl | Visual alarm grp overflow | int | 0...63
VisAlStsAct | Actual visual alarm group | int | 0...63
VisAlSts1 | Visual alarm group status1 | int | 0...63
VisAlSts2 | Visual alarm group status2 | int | 0...63
VisAlSts3 | Visual alarm group status3 | int | 0...63
VisAlSts4 | Visual alarm group status4 | int | 0...63
VisAlSts5 | Visual alarm group status5 | int | 0...63
VisAlSts6 | Visual alarm group status6 | int | 0...63
VisAlSts7 | Visual alarm group status7 | int | 0...63
VisAlSts8 | Visual alarm group status 8 | int | 0...63